Additional Requirements and Information for E-Rate 
In general, the drop counts in the spreadsheets represent enough additional drops per school to end this project with 9 drops in each classroom plus a wireless AP drop in every other classroom area.   All teachers’ areas will require two data drops.  Since most teachers’ positions have one drop this will require the installation of one additional drop.

To assist in accomplishing the installation of new jacks, the following information is provided.  
1. Almost every classroom in SAISD has one (1) data drop for the teacher and three 3) for the students.  There are exceptions and some of them are below.

2. The vendor will install one additional data drop in the teacher’s area. This new drop can be co-located with the existing data drop if possible.  

3. The Vendor needs to install a data drop in the hallway area of every other classroom down the hallway.   The exact location will be determined by a vendor conducted wireless AP survey which will insure good, constant signal strength in the area.

4. The drops to be used by the students will be co-located in one or two additional locations not to exceed 5 jacks in any one location.  This can mean two additional jacks to the existing three jack cluster and/or additional clusters.

5. Exceptions and Other Special Considerations: 

a. Glenn MS – Only need an additional data drop for the teacher and the rest will be dedicated for the students because the campus already has wireless APs installed.

b. Central Freshman Campus – Include wiring and wireless connection to Old Gym

c. Lamar – All teachers already have two data drops and wireless APs installed so the jacks will be made additional student drops

d. Bowie - Eliminate the patch panel in the library mechanical room by replacing the existing eight (8) drops

e. Bonham – Replace existing five (5) drops in old 12 port patch panel and place into rack

f. Elementary Schools with new Construction and some Re-wire Work – All elementary schools except Lamar Elem have one teacher’s jack and three student jacks except in the new construction done in the last bond issue construction.  So, in addition to Wireless APs through the campus and the additional jacks in each classroom, these buildings will need to have additional jacks installed in the classroom to bring the total count up to nine.  There are also a few areas which need to be completely rewired. The identification of these building and the campuses are: All Multipurpose buildings on every elementary campus.

g. Portables – Almost all the same.  All drops are to be installed from under the floor if at all possible.


       h.  Multi-Purpose buildings - All the same except for Belaire and Crockett.  Add 


open rack if necessary.  They have only three existing drops in the Music Room.  


Install rack, do not use shelves

6.  Additional Notes
.
a.
A Cat-5e patch panel may be allowable under certain conditions, although SAISD 
requires a Cat-6 solution whenever possible.  
1.
We want a Cat-6 solution but we realize for economic reasons there will be 
exceptions
2.
We will require all Cat-6 cabling to a classroom drop to terminate in a Cat-6 patch 
panel.

3.
No Cat-6 cabling to a classroom or office data drop will terminate in a Cat-5 
patch panel.

4.
If you are re-terminating Cat-5 you can use a Cat-5 patch panel.

5.
If you are running a cable to a single Access Point (AP) such as in a library, office 
area, or a cafeteria, where you are not going to add any Cat-6 data drops or install 
a Cat-6 patch panel, you can use Cat-5e cable and terminate them in an existing 
Cat-5 patch panel.  

6.
If you have filled up a Cat-6 patch panel or panels and would have to add an 
additional Cat-6 panel only to terminate a couple Access Points (APs) you can 
terminate the APs in existing Cat-5 patch panels, if available, and test them as 
Cat-5. 

b.
A cable run includes a 15 foot drop cable for the classroom side and a 3 or 5 foot cable 
for the patch panel side, except for where there is a Hubble RE cabinet then the patch 
cable needs to be in the one foot range, because of lack of space for longer cables.
This work will also require more patch panels and equipment racks in some areas.  Though the use of 48 port switches will produce more useable space in the racks, there may not be enough space without additional racks.  The racks specified in the spread sheet for each school may not be sufficient.  Vendor needs to take this into consideration and will be required to supply any additional racks.  All additional rack space will be the responsibility of the Vendor.  See Spreadsheets

This paper is only an informational guide and should not be construed as absolutely factual in every regard.

