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SEE KY
School Light Level Survey

1.  Flip the top black switch to ON and the bottom black switch to A.   Carefully unscrew the lid off of the light sensor and complete the survey below.

2.  Be sure to hold the sensor parallel to the floor/ceiling and collect your data with the sensor about 3ft from the floor (desk level).
	
	Foot Candle (Fc) measurement
	Minimum Requirement (Fc)
	Opportunity for energy conservation?
(What is the difference between Minimum Requirement and YOUR measurement?)

	Foyer Area 
	
	25
	

	Corridor/Hallway 1
	
	25
	

	Corridor/Hallway 2
	
	25
	

	Office Space 
	
	50
	

	Teacher workroom 
	
	50
	

	Classroom  (not lab, art or computer)
	
	75
	

	Gym
	
	Elem: 50

MS/HS: 75
	

	Cafeteria
	
	50
	

	Library
	
	75
	


What area measured the highest light level?  _______________

What was the footcandle (Fc) measurement of space with highest light level?  _______
Are there opportunities for energy conservation in light levels?
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