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Mackay School District No. 182
NONINSTRUCTIONAL OPERATIONS					8110-F(1)
Safety Busing – Safety Busing Measuring and Scoring Instrument

The following form can be found at the Idaho State Department of Education website under Student Transportation and Safety Busing.
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Legal References

	

	IC § 33-1501

	IC § 33-1506

	IC § 33-1509

	IC 33-1006

	IC 33-1504

	IC 33-1515

	Other References

	Idaho State Department of Education

	ISBA Policy Services


Cross References
	Code
	Description

	8100
	Transportation

	8120
	Bus Routes, Stops, and Non-Transportation Zones
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MEASURING INSTRUMENT FOR WALKING STUDENTS

This is worksheet that can be used to determine safety busing areas.
‘School District: School:
Location of Area Rated:
Date Rated:
[Rate the following by putting a circe around the appropriate number. The higher the number, the more hazardous the walking route. | Numeric|
Score
[Vehiculas
L. Average hourly Over | 1000- | %00 | 800 ] 700 | 600 | 500 | 400 | 300 [ 200 | 100-
Jouring schoolarivat s | 1000 | so1 | sor [ 701 [ o1 [ sor |01 f301 |21 | 101 o
|departure both
Jafterncon.
Am. o g g 7 g g T 3 7 T O
o o 5 s 7 O g T 3 2 T 0
[o-Truck wraffic quring | Over 100 0075 7551 025 51 O
Jschool arrival &
[both morming &
Jafterncon.
Am. g T 3 7 T 0
o g T 3 7 T O
[-Postea uatfic speed | _ssmph | sOmph | 4smpn | @0mpn | 3smeh | 30mpn | 2smpn | 20men
7 6 s a 3 2 1 o
Pedestrian:
[ Number of pupils | Over225] 225 | 200 | 175 | 10 | 15 [ 100 | 75 | 50 | 25 0
0 | 200 | we | ast | w2 [ a1 [ s | s | 26 1 0
s 5 7 5 s . 3 2 1
[2-Grade ever Flementary Middle School/Junior High High School
0 2 o
[Roadway:
1. Width of road Wuitiane Mutiane. Twolane Twolane | Twoway, no
divided (two-way) or Twoway Twoway | street markings
highway, raised | Single-lane. No-passing, Passing
or painted wiieft turn lane:
median
Crosing [ g g 7 g g T 3 7 T 0
[Exposure tmewalking | 30 | 2730 | 2427 | 2128 | 1821 | 1518 | 2215 | o2 | 69 | 36 | 03
Jatong (in minutes) 10 s 8 7 5 s . 3 2 1 ]
[2-Shouider or sdewalk| Mo, Narrow, Narrow, Wide, Wide, | Soewalk Sidewalk
shoulderor | unpaved paved unpaved paved allway. allway
“Narrow” —under3 | sidewalk shoulder, | shoulder, | shoulder, | shoulder, | withno withno
“Wide - 3.8 feet Jnosidewalk  |nosidewalk  [nosidewalk  [nosidewalk | breaks breaks,
shoulder or
utiitystrip
o 9| & 7| s ] 4] |z2]°* g R ED
[3- Accumutative Toow | so% | so% | 0% | 0% | sox | 4% | 0% | 20% | 0% 1%
Jarea with no sidewalk | 10 ) s 7 6 s 4 3 2 1 [
Ja-Traffc control sians | No school sizns Nopavement | No traffic signals | No traficights— | Nocrossing
|mariings (score as markings Elementary Only. guard—
Jas appiicable) Elementary Only
2 2 2 2 2
Environmental: (over)
Page1of2 April1, 2019





image2.png
MEASURING INSTRUMENT FOR WALKING STUDENTS

[Environmental: (co;

inued)

1. Visual obstructions.
trees, shrubs, its,
Jeurves, buiings, etc.)

[Comments

‘Accumulative Exposure - of Walking Route
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[TOTAL RATING:
Contacted Agency or Agency or In Contact Person W/Phone Number
State Highway District
| County Roads
City Streets
| Canal Company
Developer
Property Owner
[Other:
[Comments:
Evaluator

Date Evaluated
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