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	NOTE TO EDITOR:  THIS IS A MASTER SPECIFICATION AND NEEDS TO BE EDITED TO BECOME PROJECT SPECIFIC.  PLEASE REMOVE ALL HIGHLIGHTS AND TEXT BOXES AND MAKE ALL TEXT BLACK ONCE EDITING IS COMPLETE.


SECTION 11 52 13
PROJECTION SCREENS
PART 1 – GENERAL
1.01 SUMMARY
A. [bookmark: _Int_TOin2MJv]Contractor shall provide all labor, materials, appliances, tools, and equipment necessary for a complete projection screens installation per manufacture guidelines, code regulations, as indicated in the drawings, and as specified herein.
B. Contractors shall provide all labor, materials, appliances, tools and equipment necessary for installation of projection screens.
C. Related Sections
NOTE TO EDITOR:  REVISE RELATED SPECIFICATION AS APPROPRIATE FOR SPECIFIC PROJECT REQUIREMENTS.
1. Division 01
2. Section 05 10 00:  Structural Metal Framing 
3. Section 06 10 00:  Rough Carpentry
4. Section 09 29 00:  Gypsum Board
5. Section 09 50 00: Acoustical Panel Ceilings
6. Division 26 Electrical
7. 27 41 16: Audio Visual Systems
1.2 SUBMITTALS
A. Requirements
Submit under provisions of Section 01 33 00, Submittal Procedures.Submit product data sheets. Shop Drawings: Show layouts and types of front-projection screens, Include the following:
1. Location of screen centerline relative to end of screen case.
2. Anchorage details, including connection to supporting structure for suspended units.
Location of wiring connections for electrically operated units.
3. Wiring diagrams for electrically operated units.
B. Qualifications
1. The Contractor shall be the factory authorized distributor for the branch of equipment offered and shall have been engaged in the business of supplying and installing the specified type of system for at least five years. 
2. The Contractor shall maintain a fully equipped service organization capable of furnishing adequate repair service to the equipment. The Contractor shall be financially able to provide a performance bond covering the work and the guarantee described. The Contractor shall provide the bond if requested. 
3. Work and material for cables, cable terminations and related components shall be performed by certified installers.  The installer shall be certified by the respective product manufacturers.
1.3 QUALITY ASSURANCE
A. Place HOLDER WORDING FOR FORMATING
1.4 WARRANTY
A. Manufacturer’s warranty
B. Contractor’s Installation warranty 
PART  2  – PRODUCTS
1.1 MANUFACTURER
A. Legrand AV Da-Lite Screen Company https://www.legrandav.com/products/da-lite
B. Or Approved Equal
1.2 PROJECTION SCREENS
	Classroom Conference Room, Library, and Portable Classroom
	Legrand, or Approved Equal
	AV Da-Lite – Model C with CSR, Model No. 34730 Matte White or District Approved Equal
	60” H x 96” W
(113” diagonal) (16:10)
	Wall Mounted
	Manual

	Cafeteria Small MPR
	Legrand, or Approved Equal
	Da-Lite Model C with CSR, Model No. 34730 Matte White or District Approved Equal
	60”H x 96” W (113” diagonal) (16:10)
	As Indicated on Drawings
	Manual

	Elementary and Middle School (Small)
Auditorium
	Legrand, or Approved Equal
	Da-Lite 14770L, or District Approved Equal
	208” diagonal,
110” x 176”
(16:10)
	Ceiling Mounted
	Motorized

	High School (Large) Auditorium
	Legrand, or Approved Equal
	Da-Lite Professional 
	340” diagonal,
	Ceiling Mounted
	Motorized

	
	
	Tensioned Electrol Part #27258C, or District Approved
Equal
	180” x 288”
(16:10)
	
	



A. Screen Format: Auditoriums: HDTV; All Other Locations: Wide
B. Viewing Surface: Matte white
C. Enclosure: White
D. Mounting Kit:
a. Floating mount kit is acceptable in portable classroom buildings.
b. Provide a 10” to 14” “L” bracket for projection screens installed above bookshelves in libraries.
c. Provide a 6” “L” bracket for projection screens installed in classrooms.
PART  3 – EXECUTION
1.1 INSTALLATION
A. Installation per manufacturer’s recommendations
B. Verify Screen will pull down and clear all obstructions prior to installation. 
C. Screen Location: 
1. Classroom: Location shall be on the wall designated as a primary teaching wall. Leave space to account for students sitting in chairs and teacher demonstration tables, if any.
2. Library: Locate screen as indicated on contract drawings. Verify that the screen will clear bookshelves when lowered. Leave space to account for books which may protrude from the shelves. 
3. Auditorium: Screens shall be centered on the stage and mounted on the proscenium area. Refer to drawings for exact location. Coordinate installation with stage lighting. 

	NOTE TO EDITOR:  
1. Coordinate motorized screen power requirement with electrical engineer
2. Size motorized screens accordingly to fit in the rooms. The minimum screen height shall be 1/8 at the maximum intended viewing distance, per InfoComm recommendations. 
3. Projection screens may be ceiling or wall mounted.
4. Confirm installation method at each location.
5. Coordinate projection screen with existing lighting, including stage lighting at Auditorium.
6. Where there are no suitable walls for wall mounted projectors, such as libraries, install ceiling mounted. 
7. Mount screens as high as possible in the classroom for optimal viewing. 
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