**Oak Grove School District**

**PCBs in Schools:**

**Safety Approach for Schools**

**Summary of EPA Information**

* PCB Regulations
* Oak Grove School District Based Approach
* Best Practices for Reducing Exposures
* Air Testing
* Additional Resources

**Regulations of PCBs**

PCBs are regulated by the U.S. EPA under the Toxic Substances Control Act

A few key points:

* Regulations prohibit the use of PCBs equal to or greater than 50 ppm in caulk and other non-liquid products, including continued use of products already in place
* Intact PCB-containing light ballasts are an authorized use -BUT if they leak PCBs then the spill area must be cleaned and proper disposal of the ballast is required
* Proper classification and disposal of renovation and demolition wastes containing PCBs is required under TSCA regulations
* Regulations regarding PCB use, clean-up, and disposal can be complicated - consult James Moreno, OGSD M&O Department or your EPA Regional PCB Coordinator –

Steve Armann,

PCB Program Coordinator

[armann.steve@epa.gov](mailto:armann.steve@epa.gov) or (415) 972-3352.

**Safety** **Approach to PCBs in Schools**

• PCBs were widely used in building materials from about 1950 until 1979.

• Implementing PCB Best Management Practices

• Replacement of PCB Ballasts

• Thorough cleaning of school surfaces (initial and routine)

* Testing of air for PCB concentrations

• If air concentrations are above national health guidelines then evaluate and mitigate sources.

**Best Practices for Minimizing PCB Exposure**

**First Steps:**

If the school or building was built or renovated between 1950 and 1979 there are several steps schools can take to reduce potential exposure until it can be determined with certainty if PCBs are present:

*  Review and evaluate general cleaning practices to ensure the cleanliness of classrooms and avoid dust accumulation.
*  Ensure ventilation systems are operating as designed
*  Clean frequently to reduce dust and residue inside buildings
*  Use a wet or damp cloth or mop to clean surfaces
*  Use vacuums with high-efficiency particulate air (HEPA) filters
*  Do not sweep with dry brooms; minimize the use of dusters
*  Wash children's hands with soap & water often, particularly before eating
*  Wash children's toys often
*  Wash hands with soap and water after cleaning

**Fluorescent and High Intensity Light Ballasts:**

 EPA recommends replacement of lights having PCB-containing ballasts. Review maintenance records to determine if PCB-flourescent light ballasts have been replaced.

 Benefits include:

*  A reduction of PCBs in the air
*  Reduced disruption and cost in responding to smoking/leaking ballasts
*  Expected reduction in energy consumption
*  Long-term cost savings when replaced with more energy efficient lighting
*  Improved classroom lighting

**Caulk and Other PCB-Containing Materials:**

Consider air testing as a way to determine **if PCBs are present above indoor air public health levels**; if so:

 Conduct Testing to identify potential sources of PCBs.

 Encapsulation or barriers may be considered as short-term

measures; in the long term encapsulants are not effective for caulk with levels above a few hundred ppm

 Remove PCB-containing caulk and other known primary source materials from the building to help lower air concentrations

 Removal must be performed by qualified contractors and steps taken to minimize the spread of dust and vapors

 Re-test the air to verify successful reduction in levels; if levels in air are not reduced below public health levels, remediation and follow-up testing may be needed

**PCB Air Testing**

**PCBs in Air**

There are no regulatory standards for PCB concentrations in indoor air.

EPA has developed recommended public health levels for different age groups that are anticipated to keep PCB exposures below the “reference dose” from the combined exposures at schools and from other sources.

For more information contact: James Moreno, OGSD M&O Department at 408-647-1265 or

EPA Region 9’s PCB Coordinator:

Steve Armann,

PCB Program Coordinator

[armann.steve@epa.gov](mailto:armann.steve@epa.gov) or (415) 972-3352.

**Public Health Levels of PCBs in School Indoor Air (ng/m3)**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Age 1-<2** | **Age 2-<3** | **Age 3-<6** | **Age 6-<12**  **Elementary School** | **Age 12-<15**  **Middle School** | **Age 15-<19 High School** | **Age 19+ Adult** |
| **70** | **70** | **100** | **300** | **450** | **600** | **450** |
|  |  |  |  |  |  |  |

*http://www.epa.gov/epawaste/hazard/tsd/pcbs/pubs/caulk/maxconcentrations.htm*

**Get Professional Advice and Information:**

Remediating PCBs in buildings can be challenging

Contact your EPA PCB Coordinator –Steve Armann

Read EPA information

Work with certified contractors experienced in PCB assessment and remediation in buildings

**Additional Resources**

U.S. EPA. Current Best Practices for PCBs in Caulk Fact Sheet – Testing in Buildings

<http://www.epa.gov/pcbsincaulk/caulktesting.htm>

U.S. EPA. How to Test for PCBs and Characterize Suspect Materials

<http://www.epa.gov/epawaste/hazard/tsd/pcbs/pubs/caulk/guide/guide-sect3.htm>

U.S. EPA. Steps to Safe Renovation and Abatement of Buildings that Have PCBContaining

Caulk

<http://www.epa.gov/epawaste/hazard/tsd/pcbs/pubs/caulk/guide/index.htm>

U.S. EPA. Contractors: Handling PCBs in Caulk During Renovation

<http://www.epa.gov/epawaste/hazard/tsd/pcbs/pubs/caulk/caulkcontractors.htm>

U.S. EPA. Management, Cleanup, and Disposal of PCB Wastes

<http://www.epa.gov/epawaste/hazard/tsd/pcbs/index.htm>

U.S. EPA. Fact Sheets for Schools and Teachers About PCB-Contaminated Caulk

<http://www.epa.gov/pcbsincaulk/caulkschoolkit.htm>

U.S. EPA. PCBs in Schools Research

<http://www.epa.gov/pcbsincaulk/caulkresearch.htm>

CDC-ATSDR. Toxicological Profile for Polychlorinated Biphenyls (PCBs).

<http://www.atsdr.cdc.gov/toxprofiles/tp.asp?id=142&tid=26>

Approved by the Oak Grove School District Safety Committee on February 24, 2015. The plan was reviewed and updated August 2015, August 2016, August 2017, August 2018 and June 2019.