1. **GENERAL**
	1. **SECTION INCLUDES**
		1. Miscellaneous specialty items applicable to Work and not specified under individual technical sections.
	2. **SUBMITTALS**
		1. Shop drawings and product data for all components, hardware and accessories under provisions of Division 1, General Requirements. Show construction and fabrications details, procedures, layout and erection diagrams, anchorages and pertinent information for specified specialty item.
		2. Samples sufficiently sized to illustrate clearly all sizes, available colors, materials, patterns and finishes.
		3. Manufacturer's installation instructions and maintenance recommendations under provisions of Division 1, General Requirements.
	3. **FIELD MEASUREMENTS**
		1. Verify site conditions. Obtain accurate dimensions of openings, levels, locations and arrangements of embedded and concealed anchorages. Report discrepancies between drawings and field dimensions to Architect before commencing work.
2. **PRODUCTS**
	1. **SPECIALTY ITEMS**
		1. MONEY SAFE**,**
			1. IN-FLOOR MODEL
				1. Floor Safe, 14-1/8 inches high, 12-3/4 inches wide, 17-1/2 inches deep, 1/4 inch thick steel walls and 1/2 inch steel plate door, UL Listed, "E" Rating, combination and keyed operation.
				2. Acceptable Manufacturers

(1) Merlo Safe Huskey Vault, Tustin, CA.

* + - 1. Sportsman Steel Safe, Long Beach CA.
			2. Hayman Safe Company, Oviedo, FL.
		1. KNOX BOX
			1. Manufacturer: The Knox Co., Phoenix, AZ.
			2. Model: 3200 surface-mounted or 3200-R recessed as required, capacity 10 keys and access cards and tamper switch installed
			3. Finish: Polyester powder coat, black.
			4. Confirm location with Local Fire Authority prior to installation.
1. **EXECUTION**
	1. **INSTALLATION**
		1. Install equipment specialties according to manufacturer's recommended procedures.

**END OF SECTION**