|  |  |  |
| --- | --- | --- |
| **QUANTITY** | **EQUIPMENT DESCRIPTION** | **MODEL #** |
| 2 | Beverage Air Milk Cooler | SMF58 |
| 12 | Carter Hoffmann heated Holding Cabinet w/Dutch doors | HBU16 |
| 1 | Carter Hoffmann Refrigerated Server w/baskets – Height 36” – 1 each drop down end shelf + add stainless steel plate rest w/drop down brackets 7” – 18 gauge stainless steel on all servers 3” casters | FS-C-63 |
| 1 | Carter Hoffmann Solid Top Utility Server Height 36” – 1 each drop down end shelf + add stainless steel plate rest w/drop down brackets 7” – 18 gauge stainless steel on all servers 3” casters | FSMC54 |
| 1 | Carter Hoffmann Hot Server w/ baskets – Height 36” + add stainless steel plate rest w/drop down brackets 7” – 18 gauge stainless steel on all servers 3” casters | FS-H-63 |
| 1 | Edlund Manual Can Opener | #1 |
| 4 | Edlund NSF Electric Can Opener | #270 |
| 2 | Cleveland Convection Steamer Dbl Stacked | 24-CDP-10 |
| Multiple | Metro ShelvingSuper Adjustable Erecta Shelf to surround all wall of storeroom on casters not to exceed height of door clearance |  |
| 5 | Traulsen 3 Door Refrigerator – Reach-In full doors | RHT 332WUT120 volt |
| 5 | Traulsen 3 door Freezer – Reach–Infull doors | RLT-332WUT208-230 volt |
| 2 | Vulcan Open Burner Heavy Duty Gas RangeSnorkel convection oven in place of standard over, stainless steel side, stainless steel back finishing panel, common front top ledge, 1 5/8 stainless steel toe base 31 5/8 working height, set of 4-5” casters two locking, cooling fan for snorkel raised rear burners, gas shut off valve, gas pressure regulator, flexible gas hose w/quick disconnect & restraining device | GH6 |
| 1 | Hood system to cover all oven, steamers, stoves & dishmachines |  |
| 1 | Stero Warewasher | U-31AC |

**SNACK BAR**

|  |  |  |
| --- | --- | --- |
| **QUANTITY** | **EQUIPMENT DESCRIPTION** | **MODEL #** |
| 12 | Samco Racks |  |
| 1 | Globe Two Speed Automatic Slicer | 3850 |
| 4 | Glo Ray Portable Foodwarmers | GRFFBL |
| 4 | Vulcan Dbl Deck Gas Convection Ovenw/casters, flexible gas hose w/quick disconnect & restraining device | SG44D |
| 1 | Walk-In Refrigeration (20X24)w/shelves on locking wheels on 3 walls – kool star – HEIGHT OF SHELVES SHOULD CLEAR THE DOOR HEIGHT – Kool Star |  |
| 1 | Walk-In Freezer (24x24)w/shelves on locking wheels on 3 walls – Height of shelves should clear the door height - Kool Star |  |

|  |  |  |
| --- | --- | --- |
| 3 | Carter Hoffmann Refrigerated Server | FS-C-50 |
| 3 | Carter Hoffmann Hot Server | FS-H-50 |
| 1 | Cleveland Tilting SkilletsHydraulic hand tilt w/quick lowering feature hot & cold water, pre rinse spray head w/hose, food strainer for pouring spout, celsius temperature dial | SGM-40-TR |
| 3 | Cleveland Steam Jacketed kettlesPan carrier, flow diverter, food strainer, kettle markings, drain strainers. Faucet mounting, bracket, spring assisted hinged rotatable domeck, stainless steel cover, hot & cold water faucet w/serving sprout | KGL-80-T |
| 2  | Hobart MixerStainless steel bowl, “B” flat beater, stainless steel “B” beater, “C” wing whip “D” wire whip, “D” dough hook “P” pastry knife, “I” heavy duty wire whip | L-800 |
| 2 | Ice Machine – Manitowoc | Q-1000 |
| 2 | Insinkerator Commercial Disposer | SS-300 |

**END OF SECTION**