1. **GENERAL**
   1. **SECTION INCLUDES**
      1. Laundry appliances.
      2. Related Sections
         1. Division 15, Mechanical: Gas, water, waste and duct connections.
         2. Division 16, Electrical: Electrical connections.
   2. **QUALITY ASSURANCE**
      1. Use only skilled workmen who are thoroughly trained and experienced in the necessary crafts.
   3. **SUBMITTALS**
      1. Product data.
      2. Color samples.
      3. Meet the applicable requirements of Section 01700.
         1. Furnish one manufacturer’s extended warranty and one instructions brochure for each appliance furnished.
2. **PRODUCTS**
   1. **APPLIANCE MANUFACTURES**
      1. Major appliances to be furnished shall be from one manufacture. General Electric Inc. was used as the basis of quality and performance for this specification.
         1. General Electric.
         2. Whirlpool Corporation, Benton Harbor, MI.
         3. Thermador Corporation, Huntington Beach, CA.
         4. Or equal.
      2. See manufacturers and models indicated on Drawings

**2.02 FINISH**

**A.** White

1. **EXECUTION**
   1. **INSPECTION**
      1. Examine the substrates and conditions under which work of this section will be performed. Do not proceed until unsatisfactory conditions detrimental to timely and proper completion of the work have been corrected.
   2. **PREPARATION**
      1. Coordinate the installation of adjoining surfaces and utility rough-ins with the other trades involved.
   3. **INSTALLATION**
      1. Install equipment in strict accordance with the manufacturer’ installation drawings and instructions, the approved shop drawings, and with applicable codes and regulations
   4. **ADJUSTMENT**
      1. Upon completion of installation and hook-up of equipment, in the presence of the Owner, put each item through a complete operating cycle. Verify that equipment is properly operating. Verify that trim is in place.
      2. Adjust components as necessary to ensure continued proper operation. Remove labels from equipment.
   5. **CLEANING**
      1. Remove packing debris.
      2. Remove all labels and clean interior and exterior surfaces of each appliance.
   6. **SCHEDULE**

ITEM MODEL (General Electric.) VOLTAGE REQUIRED

Clothes Washer #GFWH 2405 LMS 120V

Clothes Dryer #GFDS 355 GLMS (Gas) 120V

Clothes Dryer #GFDS 355 ELMS (Ele.) 240v

Range 30” #JGBS 07DETWW (Gas) 120v

Range 30” #CS975SDSS (Ele.) 240V

Refrigerator #PTS25LHSWW 120V with Water Supply

Dishwasher #GLDA 690PWW 120V

Microwave #JE 1440WF 120V

**END OF SECTION**