PART 1 - GENERAL

* 1. SUMMARY
		1. Principal Work Items Are:
			1. Concrete parking bumpers at accessible parking stalls and where indicated on the drawings.
		2. Related Work:
			1. Pavement Marking: Section 32 17 23.
			2. Asphaltic Concrete Paving: Section 32 12 16.
	2. REFERENCE

Requirements in Addenda, Alternates, Conditions, and Division 1 collectively apply to this work.

* 1. SUBSTITUTIONS

Only written approval of the Architect, by Addenda or Construction Change Document, will permit substitutions for materials specified: Refer to Section 01 25 13 Product Options and Substitutions.

PART 2 - PRODUCTS

* 1. MATERIALS
		1. Bumpers:
			1. Acceptable Manufacturers:
				1. E.K. Sheefer & Sons, Paramount, California.
				2. Other Manufacturers: As accepted by Architect.
			2. Type: Pre-cast reinforced concrete, with fastening holes each end.
			3. Lengths: 4' typical at Accessible parking stalls; other lengths as noted.
		2. Anchor Pins: #5 rebar x 2'-0" long (two minimum per bumper).

PART 3 - EXECUTION

3.01 INSTALLATION

Accurately layout locations. Securely anchor in place with anchor pins driven in holes.

END OF SECTION