PART 1 - GENERAL

* 1. SUMMARY
     1. Principal Work Items Are:
        1. Concrete parking bumpers at accessible parking stalls and where indicated on the drawings.
     2. Related Work:
        1. Pavement Marking: Section 32 17 23.
        2. Asphaltic Concrete Paving: Section 32 12 16.
  2. REFERENCE

Requirements in Addenda, Alternates, Conditions, and Division 1 collectively apply to this work.

* 1. SUBSTITUTIONS

Only written approval of the Architect, by Addenda or Construction Change Document, will permit substitutions for materials specified: Refer to Section 01 25 13 Product Options and Substitutions.

PART 2 - PRODUCTS

* 1. MATERIALS
     1. Bumpers:
        1. Acceptable Manufacturers:
           1. E.K. Sheefer & Sons, Paramount, California.
           2. Other Manufacturers: As accepted by Architect.
        2. Type: Pre-cast reinforced concrete, with fastening holes each end.
        3. Lengths: 4' typical at Accessible parking stalls; other lengths as noted.
     2. Anchor Pins: #5 rebar x 2'-0" long (two minimum per bumper).

PART 3 - EXECUTION

3.01 INSTALLATION

Accurately layout locations. Securely anchor in place with anchor pins driven in holes.

END OF SECTION