
554.108 Inspection - Water Heater
(1) The inspection requirements of this chapter apply only to boilers located in public assembly locations. A potable hot water supply boiler with a heat input of 200,000 British thermal units (Btu) per hour and above, up to a heat input not exceeding 400,000 Btu per hour, is exempt from inspection, but must be stamped with the A.S.M.E. code symbol "HLW" and the boiler's A.S.M.E data report must be filed as required under s. 554.103(2).
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