ADDENDUM #1
DATED ISSUED: SEPTEMBER 9, 2025
FOR THE PROJECT:

RFP For 
REPLACEMENT OF BOILERS at WASHINGTON PRIMARY SCHOOL
DATED AUGUST 28, 2025

This addendum is submitted to answer questions received from prospective bidders by email and verbally during the mandatory walk-through on-site September 8, 2025.
Number 1- Emailed questions
1. Is a bid bond required? And if so what %?  Answer - No
2. Is a project schedule required with the bid?  Answer - No, it is required at the time of contract.
3. What is the retainage?  Answer - 5%
4. What are the daily liquidated damages?  Answer - For delay in completion, $1,000; a reasonable completion date will be mutually decided at the time of contract.
5. How many copies of the bid should we submit? Answer - 1
6. Is this project CHRO? Answer - Yes, if the cost exceeds $100,000 
7. Are permit fees waived?  Answer – There is no guarantee of waiving the fees; please identify and include all applicable fees in the proposal as an allowance.
8. Are we required to provide preventative maintenance once the job is done? If so, for how long? This would be separate from our 1 Year Workmanship Warranty. Answer - Please offer this as an alternate option. 
Number 2 – Questions from the mandatory bid walk through
1. Do all of the heating pipes in the boiler room need to be insulated, or just the new piping? Answer - All heating system piping copper or black iron overhead or wall mounted whether old or new needs to be insulated with the exception of any black iron piping connecting to the North wall circulating system. Insulation shall end at the joint between the copper and black iron going into the north wall circulating system. Any existing insulation can be resecured and reused if not damaged.
2. What is the heating capacity of the existing system? Answer – 4,200,000 BTU’s. The replacement boilers/burners shall have a total of 4.2 million BTU heating capacity.
3. Are the existing burners being reused and what type shall they be? Answer – No, the burners are not being reused. The existing burners are low and high fire flame capable. New burners shall be low/high fire or modulating capable.




Acknowledgement
All bidders must acknowledge receipt of this addendum by signing below and including it with their bid submittal. Failure to do so may result in the bid being considered non-responsive.

Company Name: ______________________________
Signature: ___________________________________
Date: _______________________________________



