Project: Shepaug Valley School Bituminous Concrete Driveway Paving

NOTE

The following clarifications and/or changes are hereby made in the Scope of Work for the project and are to be included in all proposals. Where conflicts arise, this addendum section shall take precedence.
The following work shall proceed per the addendum or per the Scope of Work if not mentioned in the addendum. A signed copy of the addendum must be included with the bid submission;

ADDENDUM #1:
A bidder sent an email with the following questions that are being shared with all potential bidders;
1- Is a bid bond required with the bid?
ANSWER – A bid bond is not required. However, a performance bond is required by the successful bidder for all projects in excess of $100,000.
2- Is a project schedule required with the bid?
ANSWER – Yes, both the scope of work and the contract require time lines and schedules for the project work.
3- Is a DAS prequalification’s certificate required with the bid?
ANSWER – No.
4- What is the retainage?
ANSWER – 5%.
5- What are the daily liquidated damages?
ANSWER - $1,000 per day. The district works with contractors at the onset if materials or labor timing require initial target completion dates to be adjusted.
6- How many copies of the bid would you like us to submit?
ANSWER – Two.
7- Is the project CHRO?
ANSWER – No, but please review Section 10.01 of the RFP, as well as Exhibit G for required nondiscrimination and equal opportunity compliance.
8- Are permit fees waived?
ANSWER – This cannot be assumed so please include these fees in your proposal. If we are successful in having them waived, we will expect a change order to remove them.
9- Are we required to provide preventative maintenance once the job is done? If so, for how long? This would be separate from a one-year Workmanship Warranty.
ANSWER – The scope of work does allow for the contractor to submit an annual maintenance service agreement if they chose. It is not required and the District may not engage for the service in its sole discretion.

ADDENDUM #2:
During the mandatory bid walk various questions were brought up and discussed regarding the Scope of Work. Following is a list of the questions and their answers;
1- What type and depth of mix shall be utilized for the project?
ANSWER – TWO (2) courses of Class 1 mix shall be used. Two (2) inches of binder and two (2) inches of finish coarse for a combined total Four (4) inches.
2- What is the milling depth?
ANSWER – Proposals shall include Milling to the existing base material.
3- How much gravel shall be needed?
ANSWER – Proposals shall include 100 tons of processed gravel, graded and compacted to be used as needed to finish grade the existing damaged areas of the base including the cost of trucking and installation costs. What is not needed will not be charged for.
4- Is replacement of the existing catch basin tops included in the project?
ANSWER – Yes, proposals shall include the cost of replacing the four (4) existing curb backed tops & one (1) exiting flat top including new steel grates.
5- Is the landscaping of the curb backs included in the project?
ANSWER – Yes, proposals shall include the cost of top soil, seed and hay for all disturbed lawns.


 

