Project: Washington Primary School Lockers Replacement Project

NOTE

The following clarifications and/or changes are hereby made in the Scope of Work for the project and are to be included in all proposals. Where conflicts arise, this addendum section shall take precedence.
The following work shall proceed per the addendum or per the Scope of Work if not mentioned in the addendum. A signed copy of the addendum must be included with the bid submission;

ADDENDUM #1:
A bidder sent an email with the following questions that are being shared with all potential bidders;
1- Is a bid bond required with the bid?
ANSWER – A bid bond is not required. However, a performance bond is required by the successful bidder for all projects in excess of $100,000.
2- Is a project schedule required with the bid?
ANSWER – Yes, both the scope of work and the contract require time lines and schedules for the project work.
3- Is a DAS prequalification’s certificate required with the bid?
ANSWER – No.
4- What is the retainage?
ANSWER – 5%.
5- What are the daily liquidated damages?
ANSWER - $1,000 per day. The district works with contractors at the onset if materials or labor timing require initial target completion dates to be adjusted.
6- How many copies of the bid would you like us to submit?
ANSWER – Two.
7- Is the project CHRO?
ANSWER – No, but please review Section 10.01 of the RFP, as well as Exhibit G for required nondiscrimination and equal opportunity compliance.
8- Are permit fees waived?
ANSWER – This cannot be assumed so please include these fees in your proposal. If we are successful in having them waived, we will expect a change order to remove them.
9- Are we required to provide preventative maintenance once the job is done? If so, for how long? This would be separate from a one-year Workmanship Warranty.
ANSWER – The scope of work does allow for the contractor to submit an annual maintenance service agreement if they chose. It is not required and the District may not engage for the service in its sole discretion.

ADDENDUM #2:
The following questions and statement have been submitted by a potential bidder for clarification. The answers are provided below;
1- The scope indicates “new steel ventilated lockers shall be 16 ga”. Does this mean all locker components shall be 16 ga?
ANSWER- The doors shall be 16 ga. The remaining components can be 24 ga.
2- Do you want just standard door louvers, top & bottom, 6 louvers at the top & bottom?
ANSWER- The top and bottom shall be louvered with a minimum of 6 louver openings for ventilation. The entire door does not need to be louvered.
3- Does cove base molding need to be replaced if disturbed on built in lockers or on free standing?
ANSWER- Yes, the cove base moldings need to be replaced where disturbed. 
4- There is a limited amount of wood trim used in the existing condition. Does the wood need to be replaced?
ANSWER- The wood does not need to be replaced; however, a factory-colored trim panel of steel would need to take its place to cover all voids and allow for a uniform, complete installation.
5- Are electrical or painting services required?
ANSWER- There is no electrical component within the existing locker systems and there is no requirement for any to be added. 
Painting is only required to fix or repair anything that either gets damaged by demo or can not be covered by a standard locker panel or trim component. 
6- Is the installation date a fixed date?
ANSWER- The installation date will be determined by the availability of component and systems delivery once that information is known. It is the intention of the district to get the systems replaced prior to school first day on or before August 25th of 2026. The winning bidder will be able to communicate the delivery and installation with the district that considers all aspects of the project best suiting both parties once the award letter is sent. 
7- Please confirm if all bidders are to use 2026-year pricing in their proposals.
ANSWER- Yes, 2026 contract pricing shall be used by all bidders.  If 2027 is available, please include.



