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INVITATION TO TENDER
3G Artificial Grass Pitch Resurfacing Works
Bilton School & Myton School, Warwickshire
Issued by P&E Sports in partnership with Stowe Valley Multi Academy Trust
1. Introduction
P&E Sports, in partnership with Stowe Valley Multi Academy Trust, invites suitably experienced contractors to submit a fixed price for the resurfacing of the existing full-size artificial surfaces at Bilton School and Myton School. Both schools are part of Stowe Valley Multi Academy Trust, and the works will be jointly funded by P&E Sports and the Trust. Contractors may price for one or both sites, but a separate priced schedule must be completed for each site tendered.
The works comprise the removal of the existing 3G carpet, associated base/shockpad works as specified per site, and the installation of a new 50mm 3G artificial turf surface meeting FIFA Quality standards, complete with line markings. The works also include replacing the existing floodlighting with a new LED floodlighting system at each site.
Target installation period: Summer 2027. Works at both sites are to be carried out during the school summer holiday period, with each pitch complete, tested and ready for use for the start of the autumn term in September 2027. Contractors should confirm in section 4.2 that their proposed programme, including lead-in and material supply, can be delivered within this period.
How to respond: this document is also the tender response form. Please complete the pricing schedules in section 3, the response boxes in sections 4 and 5, and the declaration in section 9, then return the completed document with any supporting documents (see section 8).
2. Scope of Works
2.1 Bilton School
1. Uplift and disposal of the existing astro turf
1. Inspection and testing of the existing shockpad, with confirmation of suitability for reuse
1. Supply and installation of new 50mm 3G artificial turf meeting FIFA Quality standards
1. Line markings: 1 x full-size pitch and 4 x cross-court markings
1. Replacement of the existing floodlighting with a new LED floodlighting system
1. All preliminaries, site set-up, welfare and management costs
2.2 Myton School
1. Uplift and disposal/recycling of the existing 3G carpet
1. Allowance for reworking of the existing dynamic base
1. Supply and installation of new 50mm 3G artificial turf meeting FIFA Quality standards
1. Line markings: 1 x full-size pitch and 4 x cross-court markings
1. Replacement of the existing floodlighting with a new LED floodlighting system
1. All preliminaries, site set-up, welfare and management costs
3. Pricing Schedules
Contractors should complete the schedules below in full. All prices should be fixed, stated in pounds sterling and exclusive of VAT. Where an item is included elsewhere in the price, please state “included” rather than leaving the cell blank.
3.1 Bilton School – Priced Schedule
	Item
	Contractor Price (£)

	Uplift and disposal of existing astro turf
	

	Inspection/testing of existing shockpad
	

	New 50mm 3G artificial turf meeting FIFA Quality standards
	

	Full-size and 4 x cross-court markings
	

	LED floodlighting upgrade
	

	Preliminaries
	

	Total excluding VAT
	


3.2 Myton School – Priced Schedule
	Item
	Contractor Price (£)

	Uplift and disposal/recycling of existing 3G carpet
	

	Allowance for reworking existing dynamic base
	

	New 50mm 3G artificial turf meeting FIFA Quality standards
	

	1 x full-size and 4 x cross-court markings
	

	LED floodlighting upgrade
	

	Preliminaries
	

	Total excluding VAT
	


4. Submission Requirements
Please complete every box in this section. Where a document is requested (e.g. data sheets, certificates), attach it and write the file name in the box.
4.1 Tenderer Details
	Company name
	

	Registered address
	

	Company registration number
	

	VAT number
	

	Contact name and position
	

	Email address
	

	Telephone number
	

	Site(s) tendered for (Bilton / Myton / both)
	



4.2 Technical Information
	Requirement
	Tenderer Response

	Proposed carpet system, including manufacturer (attach product data sheet)
	

	Confirmation that the proposed surface meets FIFA Quality standards (attach test certification)
	

	Warranties offered on the carpet and on installation
	

	Proposed programme for each site (lead-in time, earliest start date and duration on site), confirming delivery within the Summer 2027 target installation period
	

	Comparable recent projects (site, scope, value and completion date); referee details are requested in section 5.4
	

	Insurances held: public liability, employer’s liability and contract works (insurer, level of cover and expiry date)
	



5. Compliance, Sustainability & Social Value
In line with the finance requirements of Stowe Valley Multi Academy Trust, the following information must accompany every tender. Responses should be proportionate to the size of the contract: a short written statement in the response box under each heading is sufficient, with any relevant policies, plans or certificates attached and named in the box.
The confirmation at 5.1 and the referees at 5.4 are mandatory. Responses to 5.2 and 5.3 will be scored as part of the evaluation set out in section 7.
5.1 Modern Slavery & Human Trafficking
1. Written confirmation that, to the best of your knowledge, there is no modern slavery or human trafficking in your business or supply chains, including the manufacture and supply of the turf, infill and shockpad products proposed
1. A brief description of how you check this within your supply chain (e.g. supplier declarations, audits, contract terms)
1. Where your organisation is required to publish a statement under section 54 of the Modern Slavery Act 2015, a copy of or link to your latest statement
Tenderer response
	We confirm there is no modern slavery or human trafficking in our business or supply chains (please tick):
Yes ☐        No ☐
How we check our supply chain / link to Modern Slavery Act statement (if applicable):




5.2 Carbon Footprint & PAS 2080
Please set out how the carbon footprint of the works will be minimised. This may include:
1. Reuse, recycling or responsible end-of-life processing of the existing carpet and infill, confirming where it will go (waste transfer documentation to be provided on completion)
1. Reuse of the existing shockpad and base where suitable, reducing the need for new materials
1. The recycled content and end-of-life recyclability of the proposed turf and infill
1. Sourcing and transport of materials, and plant and vehicle movements to site
1. The energy saving of the proposed LED floodlighting compared with the existing system
Please also state whether your approach meets, or is aligned with, PAS 2080 (Carbon management in buildings and infrastructure). If it is not formally aligned, please say so and describe the carbon management measures you do have in place.
Tenderer response
	Carbon minimisation measures and PAS 2080 position:




5.3 Commitment to Net Zero
Please demonstrate your organisation’s commitment to achieving Net Zero, for example a Carbon Reduction Plan with a target date, an environmental policy, accreditations held (such as ISO 14001), and practical steps already taken.
Tenderer response
	Net Zero commitment:




5.4 Referees
Please provide at least two referees for comparable 3G pitch projects completed within the last five years, ideally including a school, academy trust or local authority client, using the table below.
	
	Referee 1
	Referee 2

	Name
	
	

	Role and organisation
	
	

	Email address
	
	

	Telephone number
	
	

	Project site
	
	

	Scope of works
	
	

	Contract value (£)
	
	

	Completion date
	
	



P&E Sports may contact referees as part of the evaluation.
6. Site Visits
Contractors are encouraged to visit both sites prior to submitting a price. Site visits can be arranged by contacting P&E Sports using the details below. Access will be coordinated with each school to avoid disruption to the school day.
7. Evaluation Criteria
Tenders will be evaluated by P&E Sports and Stowe Valley Multi Academy Trust on the basis of the most economically advantageous tender, using the criteria and weightings below. Each site will be evaluated separately.
7.1 Stage 1: Compliance (Pass/Fail)
The following must be provided in full. Tenders that do not meet these requirements may be excluded and not scored: the modern slavery confirmation (section 5.1); evidence of public liability, employer’s liability and contract works insurance (section 4.2); FIFA Quality certification for the proposed surface (section 4.2); two referees for comparable 3G projects (section 5.4); and the signed declaration (section 9).
7.2 Stage 2: Scored Evaluation
	Criterion
	What will be assessed
	Weighting

	Price
	The total price excluding VAT in the relevant priced schedule (section 3)
	50%

	Technical quality
	Proposed carpet system and manufacturer, FIFA Quality compliance, warranties on the carpet and installation, and the approach to the shockpad (Bilton) or dynamic base (Myton) (section 4.2)
	30%

	Experience, programme and sustainability
	Comparable recent projects and referee feedback (sections 4.2 and 5.4); a realistic programme that delivers within the Summer 2027 target installation period (section 4.2); carbon minimisation and Net Zero commitment (sections 5.2 and 5.3)
	20%

	Total
	
	100%



Price: the lowest compliant price for each site will receive the full 50%. Other tenders will be scored in proportion: (lowest price ÷ tendered price) × 50. The evaluated price is the total for the site, including the LED floodlighting upgrade.
Quality: responses to each quality criterion will be scored from 0 to 5 (0 = no response or unacceptable; 1 = poor; 2 = weak; 3 = satisfactory; 4 = good; 5 = excellent) and converted to the weighting shown. Abnormally low prices may be queried before evaluation is completed.
8. Tender Return
Please return this document, fully completed and signed, together with any supporting documents, by email to info@pandesports.com no later than:
12 noon, Friday 20 November 2026
Please use the email subject line “Tender – 3G Resurfacing – Bilton & Myton – [Company Name]” and attach the completed document (Word or PDF) and supporting documents. Receipt of each tender will be acknowledged by email.
Clarification questions should be emailed to the same address by 12 noon, Friday 6 November 2026. Late or incomplete tenders, including those without the mandatory information in section 5, may not be considered.
P&E Sports is not bound to accept the lowest or any tender. Any queries raised during the tender period will be answered in writing, with responses circulated to all tenderers where relevant.
9. Declaration
We confirm that we have read and understood this invitation to tender; that the prices in section 3 are fixed, stated in pounds sterling, exclusive of VAT and will remain valid for 90 days from the tender return date; and that the information provided in this response is complete and accurate.
	Signed
	

	Name
	

	Position
	

	Company
	

	Date
	



10. Contact
Dave Phelan
P&E Sports
info@pandesports.com
07561716724 
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