|  |  |  |
| --- | --- | --- |
| **QUANTITY** | **EQUIPMENT DESCRIPTION** | **MODEL #** |
| 2 | Beverage Air Milk Cooler | SMF58 |
| 6 | Carter Hoffmann heated Holding Cabinet w/Dutch doors | HBU16 |
| 1 | Carter Hoffmann Refrigerated Server w/baskets – Height 36” – 1 each drop down end shelf + add stainless steel plate rest w/drop down brackets 7” – 18 gauge stainless steel on all servers 3” casters | FS-C-63 |
| 1 | Carter Hoffmann Solid Top Utility Server Height 36” – 1 each drop down end shelf + add stainless steel plate rest w/drop down brackets 7” – 18 gauge stainless steel on all servers 3” casters | FSMC54 |
| 1 | Carter Hoffmann Hot Server w/ baskets – Height 36” + add stainless steel plate rest w/drop down brackets 7” – 18 gauge stainless steel on all servers 3” casters | FS-H-63 |
| 1 | Edlund Manual Can Opener | #1 |
| 2 | Edlund NSF Electric Can Opener | #270 |
| 1 | Cleveland Convection Steamer Dbl Stacked | 24-CGM-200 |
| Multiple | Metro Shelving  Super Adjustable Erecta Shelf to surround all wall of storeroom on casters not to exceed height of door clearance |  |
| 2 | Traulsen 3 Door Refrigerator – Reach-In  full doors | RHT 332WUT  120 volt |
| 2 | Traulsen 3 door Freezer – Reach–In  full doors | RLT-332WUT  208-230 volt |
| 1 | Vulcan Open Burner Heavy Duty Gas Range  Snorkel convection oven in place of standard over, stainless steel side, stainless steel back finishing panel, common front top ledge, 1 5/8 stainless steel toe base 31 5/8 working height, set of 4-5” casters two locking, cooling fan for snorkel raised rear burners, gas shut off valve, gas pressure regulator, flexible gas hose w/quick disconnect & restraining device | GH6 |
| 1 | Hood system to cover all oven, dishmachines & stoves |  |
| 1 | Hobart Warewasher | AM-14TC |
| **QUANTITY** | **EQUIPMENT DESCRIPTION** | **MODEL #** |
| 6 | Samco Racks |  |
| 1 | Globe Two Speed Automatic Slicer | 3850 |
| 4 | Glo Ray Portable Foodwarmers | GRFFBL |
| 2 | Vulcan Dbl Deck Gas Convection Oven  w/casters, flexible gas hose w/quick disconnect & restraining device | SG44D |
| 1 | Walk-In Refrigeration (10x12”)  w/shelves on locking wheels on 3 walls – kool star |  |
| 1 | Walk-In Freezer (12x12”)  w/shelves on locking wheels on 3 walls – kool star |  |

**SNACK BAR**

|  |  |  |
| --- | --- | --- |
| **QUANTITY** | **EQUIPMENT DESCRIPTION** | **MODEL #** |
| 3 | Carter Hoffmann Refrigerated Server | FS-C-50 |
| 3 | Carter Hoffmann Hot Server | FS-H-50 |
| 1 | Ice Machine – Manitowoc | Q-800 |
| 1 | Insinkerator Commercial Disposer | SS-200 |

**END OF SECTION**